
**PART-1**All done in the Services Tab of the DHCP Server

**PART-2  
Step-1:**R1>en  
R1>conf t  
R1(config)#interface gigabitEthernet 0/0  
R1(config-if)#ip helper-address 192.168.60.253  
R1(config-if)#exit  
R1(config)#exit  
R1#exit

**Step-2:** Done in PC1’s IP Configuration mode from Desktop

**PART-3**

**Step-1:**

From the web browser of the desktop of PC1 typed the addresses cisco.com and publicsite.com. The results are as following:  
******